**BOBCAT FENCE HAZARD TREE CLUSTER REMOVAL**

* Target dead standing trees within 1.5 tree lengths of the fence line (only target tree clusters identified with a green asterisk on the map)
* Dead standing trees shall be felled away from the fence, delimbed and bucked if necessary.
* Lop and scatter limbs and material.
* Pull back all dead and down material at least 10 feet from fence line.
* Work with BIFO fuels specialist or fuels technician to authorize access through private land.