

1. Double-click the file v:\drs\apps\drsmanager\drsmanager.exe.



1. In the startup screen that appears pick the DESTINATION drive letter, wait for the red text in the lower left to stop running, then click CUSTOMIZE.



1. Follow the 5 steps in the DRSmanager wizard:
	1. Choose to UPDATE/BUILD a DRS.
	2. Confirm the source (V) and destination drives are correct, or change them.
	3. Click Selection Criteria to show a map of MN, then hold [shft] and click on counties to include.
	4. Click Applications and Extras and choose all the checkboxes.
	5. Click a layer name to read its description in the lower right corner. Check a box to include the layer. To toggle all the boxes on or off, hold [shft] and click a checkbox.
2. Click RUN COMPLETE UPDATE to begin the copy process. The window can be moved, but not minimized, during the copy. Expect a copy rate of 4-6 gigabytes /hr.



1. Click OK to the message popup that says “DRS UPDATE COMPLETE”.
2. Close the DRSmanager program.