|  |  |  |  |
| --- | --- | --- | --- |
| **Incident Name:**SodaID-BOD-000889 | **IR Interpreter(s):**Bob Brantlinger | **Local Dispatch Phone:**ID-BDC -208-384-3398 | **Interpreted Size:**283,400 (from Incident)**Growth last period:**-0- |
| **Flight Time:**2100(MDT)**Flight Date:**08/18/2015 | **Interpreter(s) location:**Durango, Colorado**Interpreter(s) Phone:**970-769-6551 | **GACC IR Liaison:**Tim Stauffer**GACC IR Liaison Phone:**208-384-3376 | **National Coordinator:**Tom Mellin**National Coord. Phone:**208-387-5381 |
| **Ordered By:**Amy Ham | **A Number:**101 | **Aircraft/Scanner System:**144z / Phoenix | **Pilots/Techs:**Johnson-Lowry/Kaz |
| **IRIN Comments on imagery:** **2 passes, ortho and color. Raw heat. Clear.**  | **Weather at time of flight:**Clear, scattered ground moisture | **Flight Objective:**Map Heat Perimeter, Intense Heat, Scattered Heat, Isolated Heat Sources |
| **Date and Time Imagery Received by Interpreter:**08/16/2015 – 2130(PDT)  | **Type of media for final product:**shapefiles, KMZ,PDF’s, IR log **Digital files sent to:****/incident\_specific\_data/great\_basin/2015\_Incidents/2015\_Soda/IR/20150818** |
| **Date and Time Products Delivered to Incident:**08/16/2015 – 2230(PDT) |
| **Comments /notes on tonight’s mission and this interpretation:****Started interpretation using GIS perimeter from incident.** **IR flight coverage was eastern 2/3rds of Incident provided perimeter. .** **No Intense Heat.****No Scattered Heat.****Few visible heat sources were visible on either the ortho or color scans.****61 heat trips were captured over the 3 passes using raw heat file.** **South of Wilson Peak and Soldier cap peaks contained the majority.** **2 points are located ~ ½ mile inside eastern perimeter, upon inspection they appear to be a power substation on Wilson Cemetery Road.** **Another 2 isolated Heat point ~1/2 mile from perimeter are located on the southern perimeter near Bog Hole spring.****All were mapped and placed in the isolated heat sources shape file.**  |