|  |  |  |  |
| --- | --- | --- | --- |
| **Incident Name:**Norton**Incident ID:**ID-SCF-022139 | **IR Interpreter(s):****E. Trout****IRIN email:**gis@owyheeair.com | **Local Dispatch Phone:**Central Idaho Dispatch208-756-5157 | **Interpreted Size:****8,375 acres****Growth last period:**1,911 interpreted acres |
| **Flight Time:**2138 MDT**Flight Date:**2022-09-08 | **Interpreter(s) location:**Nampa, ID**Interpreter(s) Phone:**(208) 442-5405 | **GACC IR Liaison:**Nate Yorgason**GACC IR Liaison Phone:**435-590-1107 | **National Coordinator:**Tom Mellin**National Coord. Phone:**505-842-3845 |
| **Ordered By:**Dale Farrand | **A Number:**A-40 | **Aircraft/Scanner System:**N17ZX/ TK-7 | **Pilots/Techs:**C. Holley / K. Hanks |
| **IRIN Comments on imagery:**good data  | **Weather at time of flight:**Clear | **Flight Objective:**IR heat perimeter and heat sources |
| **Date and Time Imagery Received by Interpreter:**0010 MDT 2022-09-08 | **Type of media for final product:**IRIN Daily Log, Shapefiles, File Geodatabase, KML, PDF Maps**Digital files sent to:**[https://ftp.nifc.gov/public/incident\_specific\_data/](https://ftp.nifc.gov/public/incident_specific_data/great_basin/2021_Incidents/)great\_basin/2022\_Incidents/2022\_Norton/IR/20220908 **Emailed to:**fire@owyheeair.com, sm.fs.idcic@usda.gov, sm.fs.gbc\_cod@usda.gov  |
| **Date and Time Products Delivered to Incident:**0300 MDT 09/09/2022 |
| **Comments /notes on tonight’s mission and this interpretation:****Fire has continued to grow, the northeast and southeast fingers extending further to the northeast and southeast, respectively. The northeast finger has sprouted a few spot fires just south of the national forest boundary, as well as growing west, the perimeter sitting about 1 mile east from Norton Lake. The southeast finger is extending east along the Ramey Hill ridge, ending between the eastern edge of the White Creek and the top of Jack Creek drainages. The western perimeter has grown as well, with a fingers extending into the Canyon Creek and Prospect Creek drainages.** |