|  |  |  |  |
| --- | --- | --- | --- |
| **Incident Name:**  Woodtick  ID-SCF-022097 | **IR Interpreter(s):**  Chad Horman  [chad.horman@usda.gov](mailto:chad.horman@usda.gov) | **Local Dispatch Phone:**  Central Idaho Dispatch  208-758-5157 | **Interpreted Size:**  38 Acres  **Growth last period:**  3 Acres |
| **Flight Time:**  2205 MDT  **Flight Date:**  7/18/2022 | **Interpreter(s) location:**  Cedar City, UT  **Interpreter(s) Phone:**  435-592-5175 | **GACC IR Liaison:**  Nathan Yorganson  **GACC IR Liaison Phone:**  Work – (208) 557-5785  Cell – (208) 557-5826 | **National Coordinator:**  Tom Mellin  **National Coord. Phone:**  Work – (505) 842-3846  Cell – (505) 301-8176 |
| **Ordered By:**  ID-SCF | **A Number:**  A-6 | **Aircraft/Scanner System:**  King Air 149Z/Phoenix | **Pilots/Techs:**  Pilots: Boyce/Johnson  Tech: Mann |
| **IRIN Comments on imagery:**  Imagery was blurry and had some streaking. | | **Weather at time of flight:**  Clear | **Flight Objective:**  Map heat perimeter, intense, scattered, and isolated heat. |
| **Date and Time Imagery Received by Interpreter:**  7/18/2022 @ 2340 MDT | | **Type of media for final product:**  Shapefiles, one geodatabase, two pdf maps, kmz file, IRIN log. IR data was posted to IRIN Edit Services (National Incident Feature Service 2022)  **Digital files sent to:**  https://ftp.wildfire.gov/public/incident\_specific\_data/great\_basin/2022\_Incidents/2022\_Woodtick/IR/20220719 | |
| **Date and Time Products Delivered to Incident:**  07/19/2022 @ 0320 MDT | |
| **Comments /notes on tonight’s mission and this interpretation:**   * Started interpretation with previous night’s (07/17/2022) IR interpreted perimeter based on data downloaded from IRIN Edit Services (IES). * Very limited perimeter growth on either of the two fires. * On the western fire there is small patches of intense heat along the north, northeast, northwest and south flanks. * Eastern fire had slight growth on the north half. Intense heat located in that small areal. * Scattered isolated heat sources were observed. * The provided geodatabase is in in WGS84 decimal degrees, so would be convenient for working in IES and IVS. * Maps and shapefiles are in NAD83 UTM 11. * Feedback is always appreciated. Please contact the interpreter at the contact information listed above. | | | |