Incident Name: Glover Fire (ID-NCF-000730)	IR Interpreter(s): Jorge Enriquez	Local Dispatch Phone: Grangeville Interagency 208-983-6800	Interpreted Size: 69 Acres Growth last period: N/A
Flight Time: 0228 PDT Flight Date: 09/04/2017	Interpreter(s) location: Petersburg, AK Interpreter(s) Phone: 907-518-4123	GACC IR Liaison: Jim Grace GACC IR Liaison Phone: 541.771.4521	National Coordinator: Jan Johnson National Coord. Phone: 208.870.5066
Ordered By: SITL: Aaron Skinner 208-926-6427 askinner@fs.fed.us	A Number: A-2	Aircraft/Scanner System: N144Z/Phoenix	Pilots/Techs: Kaz Kazimir (IR Tech) Boyce/Ramsay (Pilots)
IRIN Comments on imagery: Imagery was clear, 2 strips, image cut off western spot	Weather at time of flight Clear	Flight Objective: Map heat perimeter, intense, scattered, and isolated heat
Date and Time Imagery Received by Interpreter: 09/04/2017 0330 PDT	Type of media for final product: PDF map, KMZ, IR log and shapefiles Digital files sent to: ftp.nifc.gov/incident_specific_data/n_rockies/2017_fires/2017_Glover/IR/20170904
Date and Time Products Delivered to Incident: IR Products 9/04/2017 @ 0445 PDT
Comments /notes on tonight’s mission and this interpretation: The Glover Fire perimeter was approximately 69 acres. The majority of intense heat are found at the head of the fire on perimeters fingers (see map). The high concentrations of isolated heat sources were mapped as scattered heat to avoid isolated heat sources cluttering most of the map area (and save time). There are a total of 146 isolated heat sources: 3 scattered throughout the interior of the larger fire perimeter areas (68 acres in size) on the west and 143 heat sources found outside the fire perimeters. The isolated heat sources found outside the larger perimeter to the west has a total of 126 isolated heat sources found outside of the perimeter (a couple are found 1.3 miles south of the fire/ SW corner of Section 4). The burning areas to the east of the larger fire is composed mostly of isolated heat sources (20 isolated heat sources) outside of a perimeter that is approximately 1 acre in size. All isolated heat sources where given X/Y coordinates, so Operations may download into GPS and navigate to these areas. Please call Jorge at the number above, if you have questions or feedback.