|  |  |  |  |
| --- | --- | --- | --- |
| **Incident Name:**East Miller Cove TN-TNS-ED0048 | **IR Interpreter(s):**Elise Bowne | **Local Dispatch Phone:**TNCC423-476-9775 | **Interpreted Size:**1055 Acres**Growth last period:** 355 Acres |
| **Flight Time:**0022 EST**Flight Date:**November 20, 2016 | **Interpreter(s) location:**Denver, CO**Interpreter(s) Phone:**303-517-7510 | **GACC IR Liaison:**Melinda McGann**GACC IR Liaison Phone:**678-320-3010 | **National Coordinator:**N/A**National Coord. Phone:**N/A |
| **Ordered By:**TN-TNS (423-339-8680) | **A Number:**10 | **Aircraft/Scanner System:**N149Z/Phoenix | **Pilots/Techs:**Netcher/Boyce/Smith |
| **IRIN Comments on imagery:**Clear, but orthorectification off in areas | **Weather at time of flight:**Clear | **Flight Objective:**Map Heat Perimeter/Isolated Heat Sources |
| **Date and Time Imagery Received by Interpreter:**November 20, 2016 0135 EST | **Type of media for final product:**PDF map, x shapefiles, kmz file and IR log**Digital files sent to:**<http://ftp.nifc.gov/incident_specific_data/southern/Tennessee/2016_EastMillerCove/IR/20161120> and emailed to David Todd |
| **Date and Time Products Delivered to Incident:**November 20, 2016 0245 EST |
| **Comments /notes on tonight’s mission and this interpretation:*** Used previous night’s IR perimeter as a starting point for tonight’s IR interpretation.
* Much less heat tonight. A few smaller areas of intense heat were mapped tonight, but mostly the area showed just scattered heat.
* There appears to be an isolated area of heat outside the north edge of the heat perimeter. It is on the north/west side of a small drainage, i.e. across the drainage from the main body of the fire.
* There is an area in the middle of the heat perimeter which seems like it has not burned. It has been left out of the heat perimeter.
* The heat appears to have been kept from the structures along the NE side of the incident.
* Questions/Concerns – please contact the IRIN at 303-517-7510.
*
* This QR code, if used in PDF Maps App, should load the IR map directly to the mobile device.
 |