|  |  |  |  |
| --- | --- | --- | --- |
| **Incident Name:**El Dorado(CA-BDU-012925) | **IR Interpreter(s):**Julian Mesickmesickj@gmail.com | **Local Dispatch:**FICC (909-383-2662) | **Interpreted Size:**22,586 Acres**Growth last period:**1.9 Acres |
| **Flight Time:** 2011 (PDT)**Flight Date:** 9/24/20  | **Interpreter(s) location:**Cedar City, UT**Interpreter(s) Phone:**425-583-4091 | **GACC IR Liaison:**Kyle Felker**GACC IR Liaison Phone:**530-251-6112 | **National Coordinator:**Jan Johnson**National Coord. Phone:**801-824-5440 |
| **Ordered By:**Phillip Dye | **A Number:**294 | **Aircraft/Scanner System:**N66GW/FireMapper 2 | **Pilots/Techs:**Mandy, Atkin  |
| **IRIN Comments on imagery:**Estimated 30 ft ground error in imagery. Gaps in imagery. | **Weather at time of flight**Clear | **Flight Objective:**Map heat perimeter, intense, scattered, and isolated heat |
| **Date and Time Imagery Received by Interpreter:**09/24/20 @ 2205 (PDT) | **Type of media for final product:** pdf maps, IR log, KMZ and shapefiles**Digital files sent to:** ftp.nifc.gov/incident\_specific\_data/calif\_s/!2020\_Incidents/CA-BDF-013409\_El\_Dorado/IR/NIROPS/20200925/ |
| **Date and Time Products Delivered to Incident:**09/25/20 @ 0101 (PDT) |
| **Comments/notes on tonight’s mission and this interpretation:*** Imagery covered (116°47'50" W – 117°4'10" W) x (33°59'0" N – 34°11'40" N).
* Used perimeter from previous night’s flight as starting perimeter.
* There was one gap in the imagery roughly 2.5 mi east of the perimeter. I marked it and bundled it with the other shapefiles as “CoverageGaps”.
* All perimeter growth occurred along southern edge of northern extension of fire. There were 2 isolated heat sources outside of the perimeter in this area also.
 |