|  |  |  |  |
| --- | --- | --- | --- |
| **Incident Name:**Snake River ComplexID-CMS-000604 | **IR Interpreter(s):**Billy HarrisWd\_harris@yahoo.com | **Local Dispatch Phone:**Grangeville Dispatch 208-983-6803 | **Interpreted Size:** 51,671 acres**Growth last period:** 12,139 acres |
| **Flight Time:** 1936 PDT**Flight Date:**07/10/21 | **Interpreter(s) location:**Astoria, Oregon**Interpreter(s) Phone:**503-791-5875 | **GACC IR Liaison:****GACC IR Liaison Phone:** | **National Coordinator:**Jan Johnson**National Coord. Phone:**505-301-8167 |
| **Ordered By:**Grangeville DispatchSITL- Brett Gore973-907-4694brett\_gore@fws.gov | **A Number:**A - 4 | **Aircraft/Scanner System:**N149Z/ Phoenix | **Pilots/Techs:**Don B.Carl H. /Rob N. |
| **IRIN Comments on imagery:**Imagery looked good | **Weather at time of flight:**Clear | **Flight Objective:**Map heat perimeter, intense, scattered, and isolated heats |
| **Date and Time Imagery Received by Interpreter:** 07/10/21 @ 2258 PDT | **Type of media for final product:**Shapefiles, KMZ, PDF maps**Digital files sent to:**<https://ftp.wildfire.gov/public/incident_specific_data/n_rockies/2021_fires/2021_SnakeRiverComplex/IR/20210711>   |
| **Date and Time Products Delivered to Incident:** 07/11/21 @ 0130 PDT |
| **Comments /notes on tonight’s mission and this interpretation:**Started interpretation with IR perimeter Shovel Creek reporting 32679 acresInterpretated acres 39,278Started interpretation with IR perimeter Hoover Ridge reporting 6,853 acresInterpretated acres 12,393Shovel Creek has intense heat along areas of eastern line and scattered heat through much oof the easterperimeter interior. There are spot fires outside the southwest line and along snake river in vicinity Limestone Point, also outside northwest line in vicinity Captain John creek.Hoover Ridge has scattered heat throughout much of the western perimeter and areas in perimeter interior Bow peak. |
|   |