Incident Name: Glover Fire (ID-NCF-000730)	IR Interpreter(s): Jorge Enriquez	Local Dispatch Phone: Grangeville Interagency 208-983-6800	Interpreted Size: 236 Acres Total Glover- 2 Acres Andy’s Hump- 234 Acres Growth last period: 167 Acres
Flight Time: 2202 PDT Flight Date: 09/04/2017	Interpreter(s) location: Petersburg, AK Interpreter(s) Phone: 907-518-4123	GACC IR Liaison: Tim Stauffer GACC IR Liaison Phone: 406-529-6366	National Coordinator: Jan Johnson National Coord. Phone: 208.870.5066
Ordered By: SITL: Aaron Skinner 208-926-6427 askinner@fs.fed.us	A Number: A-	Aircraft/Scanner System: N144Z/Phoenix	Pilots/Techs: Kaz Kazimir (IR Tech) Boyce/Ramsay (Pilots)
IRIN Comments on imagery: Imagery was clear, 2 strips, image cut off western spot	Weather at time of flight Clear	Flight Objective: Map heat perimeter, intense, scattered, and isolated heat
Date and Time Imagery Received by Interpreter: 09/04/2017 0330 PDT	Type of media for final product: PDF map, KMZ, IR log and shapefiles Digital files sent to: ftp.nifc.gov/incident_specific_data/n_rockies/2017_fires/2017_Glover/IR/20170905
Date and Time Products Delivered to Incident: IR Products 9/04/2017 @ 0445 PDT
Comments /notes on tonight’s mission and this interpretation: Utilized previous night’s (9/4) IR heat perimeter as a base to start tonight's interpretation. The Glover Fire perimeter increase was approximately 1 acres. (Andy’s Hump perimeter increase was 234 acres) see totals above. The majority of intense heat are found in the Andy’s Hump fire. Last night’s imagery exhibited super-heated vapors not touching the surface (plume of fire) and intensity in every perimeter of Andy’s Hump. The high concentrations of isolated heat sources were mapped as scattered heat to avoid isolated heat sources cluttering most of the map area (and save time). There are a total of 95 isolated heat sources: None within the Glover fire perimeter and 17 scattered throughout the interior of the Andy’s Hump fire perimeter. 49 heat sources were found outside the Andy’s Hump fire perimeters and 29 outside of the Glover fire perimeter. The isolated heat sources found outside the Andy’s Hump are found just outside of the perimeter (see map). The Glover fire is composed mostly of isolated heat sources (29 isolated heat sources) outside of a perimeter that is approximately 2 acre in size. All isolated heat sources where given X/Y coordinates, so Operations may download into GPS and navigate to these areas. Please call Jorge at the number above, if you have questions or feedback.