|  |  |  |  |
| --- | --- | --- | --- |
| **Incident Name:**  Hungry Creek  ID-NCF-000619 | **IR Interpreter(s):**  Lauren Miller | **Local Dispatch**  Grangeville Interagency Dispatch  **Phone:**  2089836800 | **Interpreted Size:**  25 Acres  **Growth last period:**  NA |
| **Flight Time:**  2206 MDT  **Flight Date:**  20190830 | **Interpreter(s) location:**  Bend OR  **Interpreter(s) Phone:**  541-408-6551 | **GACC IR Liaison:**  Tim Stauffer  **GACC IR Liaison Phone:**  406-529-6366 | **National Coordinator:**  Ton Mellin  **National Coord. Phone:**  Cell 505-301-816 |
| **Ordered By:**  Lochsa RD | **A Number:**  4 | **Aircraft/Scanner System:**  N149Z/Phoenix | **Pilots/Techs:**  Mark/Mike |
| **IRIN Comments on imagery:**  Orthorectification is off ~50 feet | | **Weather at time of flight:** | **Flight Objective:**  Map heat perimeter, scattered and intense heat and isolated heat sources |
| **Date and Time Imagery Received by Interpreter:**  20190830 2220 MDT | | **Type of media for final product:**  Digital: PDF maps, zipped shapefiles, KMZ, IRlog.docx  **Digital files sent to:**  <https://ftp.nifc.gov/public/incident_specific_data/n_rockies/2019_fires/2019_HungryCreek/IR/>  Emailed to idgvc@firenet.gov | |
| **Date and Time Products Delivered to Incident:**  20190830 2300 MDT | |

**Comments /notes on tonight’s mission and this interpretation:**

No previous perimeter available. There is an estimated perimeter in WFDSS, but it is hand drawn so I did not use it as a base to begin interpretation. Orthorectification was a ~ 50 feet off; I adjusted perimeter to account for this. No intense heat. Scattered heat along all flanks, a few isolated heat sources interior.