Incident Name: Milli Fire (OR-DEF-000843)	IR Interpreter(s): Jorge Enriquez	Local Dispatch Phone: COIDC 541.316.7700	Interpreted Size: 24,079 Acres Growth last period: 53 Acres
Flight Time: 0154 PDT Flight Date: 09/07/2017	Interpreter(s) location: Petersburg, AK Interpreter(s) Phone: 907-518-4123	GACC IR Liaison: Jim Grace GACC IR Liaison Phone: 541.771.4521	National Coordinator: Jan Johnson National Coord. Phone: 208.870.5066
Ordered By: SITL: Jack Johnson 719.580.5199 jkj@amigo.net	A Number: A-104	Aircraft/Scanner System: N149Z/Phoenix	Pilots/Techs: Kuenzi (IR Tech) Netcher/White (Pilots)
IRIN Comments on imagery: Imagery was clear, 2 strips	Weather at time of flight Cloudy	Flight Objective: Map heat perimeter, intense, scattered, and isolated heat
Date and Time Imagery Received by Interpreter: 09/07/2017 0300 PDT	Type of media for final product: PDF map, KMZ, IR log and shapefiles Digital files sent to: ftp.nifc.gov/incident_specific_data/pacific_nw/2017_Incidents_Oregon/2017_MILLI_ORDEF_0843_CS/IR/20170907
Date and Time Products Delivered to Incident: IR Products 9/07/2017 @ 0400 PDT
Comments /notes on tonight’s mission and this interpretation: Utilized GISS (9/6) fire perimeter as a base to start tonight's interpretation. The Milli Fire perimeter increase was approximately 53 acres. The perimeter increase is along the southwestern edges of the fire (there are new perimeters in this area ahead of fire/ area in-between may have burned but heat was not as evident to map into & expand larger perimeter). Intense heat is also displayed along the areas of increase noted above. The high concentrations of isolated heat sources were mapped as scattered heat to avoid isolated heat sources cluttering most of the map area (and save time). There are a total of 74 isolated heat sources: 48 scattered throughout the interior of the fire perimeter and 26 heat sources found outside the fire perimeter. The isolated heat sources found outside the perimeter are found along the southwest portion of the fire and a few along the western edge. All isolated heat sources where given X/Y coordinates, so Operations may download into GPS and navigate to these areas. Please call Jorge at the number above, if you have questions or feedback. Note: The Whitewater incident to the southwest of Milli displayed a lot of intense heat. See mosaic attached.