Register with HDDS

Go to <http://hdds.usgs.gov/hdds2/>

Download Imagery

Go to <http://hdds.usgs.gov/hdds2/>

Stack Imagery

Go to the ArcToolbox, select ERDAS Image Analysis Tool, select Utilities, and select Layer Stack.

Select the image layers in the same numeric order as in the name of each file.

Display Imagery as IR

Open the display option in Arc, select band 2 for Blue, band 3 for Green, and band 4 for Red.

Subscript to RSS Feed (Optional)

Go to <http://hdds.usgs.gov/hdds2/feed/subscribe>