|  |  |  |  |
| --- | --- | --- | --- |
| **Incident Name:**Medio(NM-SNF-000532) | **IR Interpreter(s):**Julian Mesickmesickj@gmail.com | **Local Dispatch Phone:**Santa Fe (505-438-5600) | **Interpreted Size:**3,753 Acres**Growth last period:**32 Acres |
| **Flight Time:** 2009 (MDT)**Flight Date:** 09/01/20  | **Interpreter(s) location:**Cedar City, UT**Interpreter(s) Phone:**425-583-4091 | **GACC IR Liaison:**Tom Mellin**GACC IR Liaison Phone:**505-842-3845 | **National IR Coordinator:**Tom Mellin**National Coord. Phone:**505-842-3845 |
| **Ordered By:**Josh Goldstein | **A Number:**54 | **Aircraft/Scanner System:**N66GW/FireMapper 2 | **Pilots/Techs:**Mandy, Atkin  |
| **IRIN Comments on imagery:**Passes matched up well with each other and did not need correction. Blocked out in one area due to clouds. | **Weather at time of flight**Some clouds in area. Blocked out imagery in one area. | **Flight Objective:**Map heat perimeter, intense, scattered, and isolated heat |
| **Date and Time Imagery Received by Interpreter:**09/02/20 @ 0130 (MDT) | **Type of media for final product:** pdf maps, IR log, KMZ and shapefiles**Digital files sent to:** ftp.nifc.gov/incident\_specific\_data/southwest/GACC\_Incidents/2020/2020\_Medio/IR/20200902/ |
| **Date and Time Products Delivered to Incident:**09/02/20 @ 0427 (MDT) |
| **Comments/notes on tonight’s mission and this interpretation:*** Imagery covered (105°47'30" W – 105°54'10" W) x (35°45'10" N – 35°53'0" N).
* 96 acre area in imagery blocked out by clouds. Marked and bundled with shapefiles as “CoverageGaps”. This occurred in the northern part of the perimeter where there was little activity. No heat was visible bordering this area.
* Used perimeter provided by GISS as starting perimeter.
* Very little activity in northern section of perimeter.
* Majority of perimeter growth in southwestern area of perimeter.
* No intense heat in perimeter.
 |